**Prilog 2: Tehničke specifikacije**

**Naziv predmeta nabave:** Stakla za kabinu – diesel, razvoj alata i atest stakala kabine

**GRUPA 2:** Stakla za kabinu – diesel, razvoj alata i atest stakala kabine – kaljena stakla

Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena grupa predmeta nabave mora zadovoljavati te se iste ne smiju mijenjati od strane ponuditelja.

Ponuditelj popunjava samo ćelije **obilježene sivom bojom**. "PONUĐENE FUNKCIONALNOSTI“ ponuditelj popunjava definirajući karakteristike ponuđenog predmeta nabave (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđenog predmeta nabave, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“, „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“).

Stupac "NAPOMENA" ponuditelj može popuniti ukoliko smatra potrebnim.

Stupac "OCJENA (da/ne)" ponuditelj NE popunjava s obzirom na to da je stupac predviđen za ocjene Naručitelja.

Kako bi se ponuda za određenu grupu predmeta nabave smatrala valjanom, ponuđena grupa predmeta nabave mora zadovoljiti sve što je traženo u obrascu Tehničkih specifikacija za određenu grupu.

Za predmet nabave, za sve stavke/opise u kojima se eventualno traži ili navodi marka, patent, tip ili određeno podrijetlo, ponuditelj može ponuditi „jednakovrijedno“ traženom ili navedenom, ali u tom slučaju mora uz ponudu priložiti dokaze o jednakovrijednosti (katalog, potvrde proizvođača ili sl.).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **R.BR.** | **NAZIV STAVKE** | **TEHNIČKE SPECIFIKACIJE / FUNKCIONALNOSTI** | **PONUĐENE FUNKCIONALNOSTI** | **NAPOMENA** ***(ukoliko je potrebno)*** | **OCJENA** **(da/ne) *popunjava Naručitelj*** |
|  | **Razvoj i izrada alata za stakla kabine – 1 komplet** |
|  | Alati za lijevo bočno staklo kabine | Razvoj i izrada alata potrebnih za proizvodnju lijevog bočnog stakla kabine, prema RASCO crtežu lijevog bočnog stakla kabine br. 74000006Alati za nanošenje sitotiska na lijevo bočno staklo kabine moraju biti uključeni u ponudi.Količina: 1 set |  |  |  |
|  | Alati za desno bočno staklo kabine | Razvoj i izrada alata potrebnih za proizvodnju desnog bočnog stakla kabine, prema RASCO crtežu desnog bočnog stakla kabine br. 74000005Alati za nanošenje sitotiska na desno bočno staklo kabine moraju biti uključeni u ponudi.Količina: 1 set |  |  |  |
|  | **Stakla za kabinu za prototipove – 1 komplet** |
|  | Lijevo bočno staklo kabine | Proizvodnja lijevog bočnog stakla kabine prema RASCO crtežu lijevog bočnog stakla kabine br. 74000006**SPECIFIKACIJE STAKLA:**Tip stakla: kaljenoUkupna debljina stakla: 5 mmBoja: zeleno tonirano staklo, potrebno prenošenje svjetlosti minimalno 80%Sitotisak: kao što je definirano na RASCO crtežu lijevog bočnog stakla kabine br. 74000006Certifikati: prema ECE R43Količina: 5 kom |  |  |  |
|  | Desno bočno staklo kabine | Proizvodnja desnog bočnog stakla kabine prema RASCO crtežu desnog bočnog stakla kabine br. 74000005**SPECIFIKACIJE STAKLA:**Tip stakla: kaljenoUkupna debljina stakla: 5 mmBoja: zeleno tonirano staklo, potrebno prenošenje svjetlosti minimalno 80%Sitotisak: kao što je definirano na RASCO crtežu desnog bočnog stakla kabine br. 74000005Certifikati: prema ECE R43Količina: 5 kom |  |  |  |
|  | Staklo poda kabine | Proizvodnja stakla poda kabine prema RASCO crtežu stakla poda kabine br. 74000007**SPECIFIKACIJE STAKLA:**Tip stakla: kaljenoUkupna debljina stakla: 10 mmBoja: prozirno stakloCertifikati: nisu potrebniKoličina: 5 kom |  |  |  |

**Annex 2: Technical specifications**

**Procurement Title:** Cabin glasses – diesel, development of tools, single certificates for cabin glasses

**LOT 2:** Cabin glasses – diesel, development of tools, single certificates for cabin glasses – tempered glasses

Requirements defined by this Technical Specifications represent minimum requirements that the offered goods/service must meet and are not allowed to be changed by Tenderer.

**Tenderer shall complete only cells marked with gray color.** Tenderer shall complete column "OFFERED FUNCTIONALITIES" defining in detail technical specifications of offered goods (note: tenderer fills the exact specifications of offered goods, while avoiding filling the columns only with words "compliant" and "equivalent", or "yes").

The column "NOTES" tenderer can fill up if deemed necessary.

The column "RATING YES / NO" is intended for the Contracting Authority and is NOT filled in by the tenderer.

For offer to be consider as compliant, offered goods/service must meet all the requirements presented in the Technical Specifications for offered Lot.

For the subject of the procurement, for all items/descriptions which may be affixed to a trademark, patent, type or specific origin, the Tenderer may offer "equivalent" to the requested or specified, but in that case must enclose proof of equivalence (catalog, manufacturer’s certificate, etc.).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM NO.** | **ITEM** | **TECHNICAL SPECIFICATIONS / FUNCTIONALITIES** | **OFFERED FUNCTIONALITIES** | **NOTES** ***(if deemed necessary)*** | **RATING****(YES/NO)** ***(fills up the Contracting Authority)*** |
|  | **Development and production of tools for cabin glasses manufacturing – 1 set** |
|  | Tools for cabin left side glass | Development and production of tools required for cabin left side glass manufacturing, according to RASCO left side glass drawing nr. 74000006.Tools for silkscreen application on cabin left side glass must be included in offer.Quantity: 1 set |  |  |  |
|  | Tools for cabin right side glass | Development and production of tools required for cabin right side glass manufacturing, according to RASCO right side glass drawing nr. 74000005.Tools for silkscreen application on cabin right side glass must be included in offer.Quantity: 1 set |  |  |  |
|  | **Cabin glasses for prototypes – 1 set** |
|  | Cabin left side glass | Manufacturing of cabin left side glass according to RASCO cabin left side glass drawing nr. 74000006**GLASS SPECIFICATIONS:**Glass type: temperedTotal glass thickness: 5 mmColor: green toned glass, required light transmittance minimum 80%Silkscreen: as defined on RASCO cabin left side glass drawing nr. 74000006Certificates: according to ECE R43Quantity: 5 pcs |  |  |  |
|  | Cabin right side glass | Manufacturing of cabin right side glass according to RASCO cabin right side glass drawing nr. 74000005**GLASS SPECIFICATIONS:**Glass type: temperedTotal glass thickness: 5 mmColor: green toned glass, required light transmittance minimum 80%Silkscreen: as defined on RASCO cabin right side glass drawing nr. 74000005Certificates: according to ECE R43Quantity: 5 pcs |  |  |  |
|  | Cabin floor glass | Manufacturing of cabin floor glass according to RASCO cabin floor glass drawing nr. 74000007**GLASS SPECIFICATIONS:**Glass type: temperedTotal glass thickness: 10 mmColor: clear glassCertificates: none requiredQuantity: 5 pcs |  |  |  |